NAME
| DmmSurfTetNode -- custom node that performs the surftet operation

SYNOPSIS
| const MTypeId DmmSurfTetNode::id = 0x0010D486;

DESCRIPTION
| The DmmSurfTetNode custom node performs the surftet operation using as input either a single triangulated Maya polygonal mesh plus scalar thickness or a pair of triangulated Maya polygonal meshes.
  | Input attribute: "triMesh1"
  Maya attribute type: | MFnTypedAttribute (MFnData::kMesh)
  Brief name: | "tm1"
  Affects attributes: | "tetMesh"
  Typical connection: | "outMesh" of a "*_DMMtri" shape node
  Input attribute: "triMesh2"
  Maya attribute type: | MFnTypedAttribute (MFnData::kMesh)
  Brief name: | "tm2"
  Affects attributes: | "tetMesh"
  Typical connection: | "outMesh" of a "*_DMMtri" shape node
  Input attribute: "thickness"
  Maya attribute type: | MFnNumericAttribute (MFnNumericData::kDouble)
  Brief name: | "thk"
  Affects attributes: | "tetMesh"
  Typical connection: | user input from attribute editor
  Output attribute: "tetMesh"
  Maya attribute type: | MFnTypedAttribute (MFnData::kMesh)
  Brief name: | "tet"
  Affected by attributes: | "triMesh1", "triMesh2", "thickness"
  Typical connection: | "modelTetmesh" of DmmObjectNode and "tetMesh" of DmmPrepMeshNode
  Output attribute: "numTets"
  Maya attribute type: | MFnNumericAttribute (MFnNumericData::kInt)
  Brief name: | "nts"
  Affected by attributes: | None (but changes whenever "tetMesh" changes)
  Typical connection: | UI.mel script